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	Model:
	Y6

	APP:
	Yiiot

	System structure:
	Embedded Linux system, ARM chip structure

	Chip:
	AK3918E

	Resolution:
	2.0MP

	Sensor Resolution:
	1/4"GC1054、SC1245 1920*1080

	Lens:
	3.6MM

	View angle:
	80°

	Pan-tilt:
	Rotates Horizontal:355°Vertical：90°

	Preset point quantity:
	6

	Video compression standard:
	H.264/20FPS

	Video format:
	PAL

	Minimum illumination:
	0.01Lux@（F2.0，VGC ON),O.Luxwith IR

	Electronic shutter:
	Auto

	Backlight compensation:
	Support

	Noise reduction:
	2D、3D

	Led quantity:
	4PCS infrared LED、4PCS White LED

	Network:
	WIFI wireless transmission (support IEEE802.11b/g/n wireless protocol).without RJ45 port

	Network connection:
	WIFI, AP Hotspot

	Night vision
	IR-CUT switch Automatic，about 5-8meters (It varies from environment)

	
Audio:
	Built-in microphone and speaker, support two-way audio and real-time transmission. ADPCM audio compression standard, self-adapt to code stream

	Network protocol:
	TCP/IP、UDP、RTSP、HTTPDDNS、DHCP、FTP、NTP

	Alarm:
	①Motion detection and picture push	②AI Human intrusion Detection (optional)

	Storage:
	TF Card（Max 128G）；Cloud storage /Cloud disk (optional)

	Power input:
	5V/1.6A

	Work environment:
	Working temperature:-10℃ ~ + 50℃	Working Humidity: ≤95%RH
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